320
This file just needs to exist in the data folder to have sven use a webcam and hence chose the right options.
The resolution is determined by the first line of this file.
Use 640 or 320 for generic capture driver... Use 64 or 32 for Fire-i (will translate to 640 or 320 resolution.)
